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Technical Note

User-Programmable LED Template for the UR-series Universal Relay

Publication reference: GET-8494A

Copyright © 2025 GE Vernova
DESCRIPTION
The UR series of relays have 48 optional user-programmable LEDs. Each LED can be configured via the EnerVista UR Setup software (preferred method) or from the front panel display via the SETTINGS  PRODUCT SETUP  USER-PROGRAMMABLE LEDS menu. Refer to the instruction manual for additional details.


The pushbuttons provide an easy and error-free method of displaying digital information (ON, OFF) from FlexLogic™ operands. Typical applications include breaker control, autorecloser status, and setting groups activation.

TEMPLATE
The User-Programmable LED Template is shown on the following page. Click on the LED X (x = 1 to 48) text fields within each label to edit the label text. Each label should contain no more than 12 characters of text. The labels are sized to align with the LEDs.


When the custom labels are completed, save this document to a secure location before printing. For best results, print to a color printer on the GE Multilin UR-series custom LED labels.
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Figure 1: User-programmable LED template

TEMPLATE
The following procedure demonstrates how to install/uninstall the custom panel labeling.


1.
Remove the clear Lexan front cover (GE Multilin part number: 1501-0014).
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2. Pop out the LED module and/or the blank module with a screwdriver as shown below. Be careful not to damage the plastic.
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3. Place the left side of the customized module back to the front panel frame, then snap back the right side.

4. Put the clear Lexan front cover back into place.
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